**SIMULADOR DEL COMPUTADOR EASY8**

Proyecto Final de Carrera

SIMULADOR DEL COMPUTADOR EASY8

**Autor**: David Marzo Muñoz

**Director**: Antonio Martí Campoy/Alberto González Téllez

Junio 2016

Resumen

En este proyecto se debe realizar un simulador para ejecutar programas en ensamblador del computador Easy8.

A partir de un fichero de texto plano con un programa en ensamblador, debe ensamblar y codificar el programa, para posteriormente permitir la ejecución paso a paso o completa, mostrando el estado de la memoria, de las unidades funcionales del procesador y de los periféricos incorporados en un interfaz gráfico.

**Palabras clave:** No te olvides de ponerlas ☺ integer, blandit, pharetra, urna, id.

Tabla de contenidos

[1 Introduction 5](#_Toc455573361)

[2 Objective 6](#_Toc455573362)

[3 Requirements 7](#_Toc455573363)

[4 Application desi](#_Toc455573364)[[1 Introduction 5](#_Toc455573364)](#_Toc455573534)

[[2 Objective 7](#_Toc455573364)](#_Toc455573535)

[3 Requirements](#_Toc455573536)[[1 Introduction 8](#_Toc455573536)](#_Toc455573596)

[[2 Objective 9](#_Toc455573536)](#_Toc455573597)

[[3 Requirements 10](#_Toc455573536)](#_Toc455573598)

[[4 Application design 11](#_Toc455573536)](#_Toc455573599)

[[4.1 Used design patterns 11](#_Toc455573536)](#_Toc455573600)

[[4.1.1 Singleton pattern 11](#_Toc455573536)](#_Toc455573601)

[[4.1.2 Factory Pattern 11](#_Toc455573536)](#_Toc455573602)

[[4.2 Pseudo codes 12](#_Toc455573536)](#_Toc455573603)

[[4.2.1 Main - Run/Step execution 12](#_Toc455573536)](#_Toc455573604)

[[4.2.2 Instruction implementation 12](#_Toc455573536)](#_Toc455573605)

[[4.2.3 Seven Digit display 12](#_Toc455573536)](#_Toc455573606)

[[4.2.4 Pseudo code Explanations 12](#_Toc455573536)](#_Toc455573607)

[[4.3 Customization of classes 12](#_Toc455573536)](#_Toc455573608)

[[5 Environment / Programming language/Implementation 13](#_Toc455573536)](#_Toc455573609)

[[5.1 Implementations 13](#_Toc455573536)](#_Toc455573610)

[[5.1.1 Seven digit 13](#_Toc455573536)](#_Toc455573611)

[[5.1.2 Battery of 8 switches 14](#_Toc455573536)](#_Toc455573612)

[[5.1.3 Implementation of one instruction – we show here the instruction CALL 14](#_Toc455573536)](#_Toc455573613)

[[6 Configuration files 16](#_Toc455573536)](#_Toc455573614)

[[7 Assemble working 17](#_Toc455573536)](#_Toc455573615)

[[8 Known Limitations-improvements 18](#_Toc455573536)](#_Toc455573616)

[[9 Manual 19](#_Toc455573536)](#_Toc455573617)

[[9.1 Execution of Gui 19](#_Toc455573536)](#_Toc455573618)

[[1. Windows 19](#_Toc455573536)](#_Toc455573619)

[[2. Linux 19](#_Toc455573536)](#_Toc455573620)

[[9.2 Execution of assembler 19](#_Toc455573536)](#_Toc455573621)

[[1. Windows 19](#_Toc455573536)](#_Toc455573622)

[[2. Linux 19](#_Toc455573536)](#_Toc455573623)

[[10 Gui 20](#_Toc455573536)](#_Toc455573624)

[[10.1 All parts view 20](#_Toc455573536)](#_Toc455573625)

[[10.2 Editing/saving assembler/memory files 21](#_Toc455573536)](#_Toc455573626)

[[10.2.1 Open assembler file 21](#_Toc455573536)](#_Toc455573627)

[[10.2.2 Save assembler file 21](#_Toc455573536)](#_Toc455573628)

[[10.3 Memory view 23](#_Toc455573536)](#_Toc455573629)

[[10.3.1 Memory 23](#_Toc455573536)](#_Toc455573630)

[[10.3.2 Instruction cpu 23](#_Toc455573536)](#_Toc455573631)

[[10.3.3 Stack 23](#_Toc455573536)](#_Toc455573632)

[[10.4 Seven segment display 24](#_Toc455573536)](#_Toc455573633)

[[10.4.1 Battery of 8 switches 24](#_Toc455573536)](#_Toc455573634)

[[10.5 Toolbar 25](#_Toc455573536)](#_Toc455573635)

[[1.1. Gui Menu 25](#_Toc455573536)](#_Toc455573636)

[[11 Gui behaviour 26](#_Toc455573536)](#_Toc455573637)

[[11.1 File types used in the simulator 26](#_Toc455573536)](#_Toc455573638)

[[11.1.1 Files that could be used in the Simulator 26](#_Toc455573536)](#_Toc455573639)

[[11.2 How to change memory value? 26](#_Toc455573536)](#_Toc455573640)

[[12 Debugger 28](#_Toc455573536)](#_Toc455573641)

[[12.1 Step Button 28](#_Toc455573536)](#_Toc455573642)

[[12.2 Breakpoints 28](#_Toc455573536)](#_Toc455573643)

[[12.3 – Run Button 28](#_Toc455573536)](#_Toc455573644)

[[12.4 – Stop Button 28](#_Toc455573536)](#_Toc455573645)

[[13 – Easy8 instructions list 28](#_Toc455573536)](#_Toc455573646)

[[14 Appendix 30](#_Toc455573536)](#_Toc455573647)

[[14.1 Save file flow 32](#_Toc455573536)](#_Toc455573648)

[[15 CONCLUSIONS and future work 34](#_Toc455573536)](#_Toc455573649)

[[16 Index 35](#_Toc455573536)](#_Toc455573650)

[[List of pictures 36](#_Toc455573536)](#_Toc455573651)

[8](#_Toc455573536)

[[4 Application design 9](#_Toc455573364)](#_Toc455573537)

[[4.1 Used design patterns 9](#_Toc455573364)](#_Toc455573538)

[[4.1.1](#_Toc455573364)[Singleton pattern 9](#_Toc455573364)](#_Toc455573539)

[[4.1.2](#_Toc455573364)[Factory Pattern 9](#_Toc455573364)](#_Toc455573540)

[[4.2 Pseudo codes 10](#_Toc455573364)](#_Toc455573541)

[[4.2.1](#_Toc455573364)[Main - Run/Step execution 10](#_Toc455573364)](#_Toc455573542)

[[4.2.2](#_Toc455573364)[Instruction implementation 10](#_Toc455573364)](#_Toc455573543)

[[4.2.3](#_Toc455573364)[Seven Digit display 10](#_Toc455573364)](#_Toc455573544)

[[4.2.4](#_Toc455573364)[Pseudo code Explanations 10](#_Toc455573364)](#_Toc455573545)

[[4.3 Customization of classes 10](#_Toc455573364)](#_Toc455573546)

[[5 Environment / Programming language/Implementation 11](#_Toc455573364)](#_Toc455573547)

[[5.1 Implementations 11](#_Toc455573364)](#_Toc455573548)

[[5.1.1](#_Toc455573364)[Seven digit 11](#_Toc455573364)](#_Toc455573549)

[[5.1.2](#_Toc455573364)[Battery of 8 switches 12](#_Toc455573364)](#_Toc455573550)

[[5.1.3](#_Toc455573364)[Implementation of one instruction – we show here the instruction CALL 12](#_Toc455573364)](#_Toc455573551)

[[6 Configuration files 14](#_Toc455573364)](#_Toc455573552)

[[7 Assemble working 15](#_Toc455573364)](#_Toc455573553)

[[8 Known Limitations-improvements 16](#_Toc455573364)](#_Toc455573554)

[[9 Manual 17](#_Toc455573364)](#_Toc455573555)

[[9.1 Execution of Gui 17](#_Toc455573364)](#_Toc455573556)

[[1.](#_Toc455573364)[Windows 17](#_Toc455573364)](#_Toc455573557)

[[2.](#_Toc455573364)[Linux 17](#_Toc455573364)](#_Toc455573558)

[[9.2 Execution of assembler 17](#_Toc455573364)](#_Toc455573559)

[[1.](#_Toc455573364)[Windows 17](#_Toc455573364)](#_Toc455573560)

[[2.](#_Toc455573364)[Linux 17](#_Toc455573364)](#_Toc455573561)

[[10 Gui 18](#_Toc455573364)](#_Toc455573562)

[[10.1 All parts view 18](#_Toc455573364)](#_Toc455573563)

[[10.2 Editing/saving assembler/memory files 19](#_Toc455573364)](#_Toc455573564)

[[10.2.1](#_Toc455573364)[Open assembler file 19](#_Toc455573364)](#_Toc455573565)

[[10.2.2](#_Toc455573364)[Save assembler file 19](#_Toc455573364)](#_Toc455573566)

[[10.3 Memory view 21](#_Toc455573364)](#_Toc455573567)

[[10.3.1](#_Toc455573364)[Memory 21](#_Toc455573364)](#_Toc455573568)

[[10.3.2](#_Toc455573364)[Instruction cpu 21](#_Toc455573364)](#_Toc455573569)

[[10.3.3](#_Toc455573364)[Stack 21](#_Toc455573364)](#_Toc455573570)

[[10.4 Seven segment display 22](#_Toc455573364)](#_Toc455573571)

[[10.4.1](#_Toc455573364)[Battery of 8 switches 22](#_Toc455573364)](#_Toc455573572)

[[10.5 Toolbar 23](#_Toc455573364)](#_Toc455573573)

[[1.1. Gui Menu 23](#_Toc455573364)](#_Toc455573574)

[[11 Gui behaviour 24](#_Toc455573364)](#_Toc455573575)

[[11.1 File types used in the simulator 24](#_Toc455573364)](#_Toc455573576)

[[11.1.1](#_Toc455573364)[Files that could be used in the Simulator 24](#_Toc455573364)](#_Toc455573577)

[[11.2 How to change memory value? 24](#_Toc455573364)](#_Toc455573578)

[[12 Debugger 26](#_Toc455573364)](#_Toc455573579)

[[12.1 Step Button 26](#_Toc455573364)](#_Toc455573580)

[[12.2 Breakpoints 26](#_Toc455573364)](#_Toc455573581)

[[12.3 – Run Button 26](#_Toc455573364)](#_Toc455573582)

[[12.4 – Stop Button 26](#_Toc455573364)](#_Toc455573583)

[[13 – Easy8 instructions list 26](#_Toc455573364)](#_Toc455573584)

[[14 Appendix 28](#_Toc455573364)](#_Toc455573585)

[[14.1 Save file flow 30](#_Toc455573364)](#_Toc455573586)

[[15 CONCLUSIONS and future work 32](#_Toc455573364)](#_Toc455573587)

[[16 Index 33](#_Toc455573364)](#_Toc455573588)

[[List of pictures 34](#_Toc455573364)](#_Toc455573589)

[gn 8](#_Toc455573364)

[4.1 Used design patterns 8](#_Toc455573365)

[4.1.1 Singleton pattern 8](#_Toc455573366)

[4.1.2 Factory Pattern 8](#_Toc455573367)

[4.2 Pseudo codes 9](#_Toc455573368)

[4.2.1 Main - Run/Step execution 9](#_Toc455573369)

[4.2.2 Instruction implementation 9](#_Toc455573370)

[4.2.3 Seven Digit display 9](#_Toc455573371)

[4.2.4 Pseudo code Explanations 9](#_Toc455573372)

[4.3 Customization of classes 9](#_Toc455573373)

[5 Environment / Programming language/Implementation 10](#_Toc455573374)

[5.1 Implementations 10](#_Toc455573375)

[5.1.1 Seven digit 10](#_Toc455573376)

[5.1.2 Battery of 8 switches 11](#_Toc455573377)

[5.1.3 Implementation of one instruction – we show here the instruction CALL 11](#_Toc455573378)

[6 Configuration files 13](#_Toc455573379)

[7 Assemble working 14](#_Toc455573380)

[8 Known Limitations-improvements 15](#_Toc455573381)

[9 Manual 16](#_Toc455573382)

[9.1 Execution of Gui 16](#_Toc455573383)

[1. Windows 16](#_Toc455573384)

[2. Linux 16](#_Toc455573385)

[9.2 Execution of assembler 16](#_Toc455573386)

[1. Windows 16](#_Toc455573387)

[2. Linux 16](#_Toc455573388)

[10 Gui 17](#_Toc455573389)

[10.1 All parts view 17](#_Toc455573390)

[10.2 Editing/saving assembler/memory files 18](#_Toc455573391)

[10.2.1 Open assembler file 18](#_Toc455573392)

[10.2.2 Save assembler file 18](#_Toc455573393)

[10.3 Memory view 20](#_Toc455573394)

[10.3.1 Memory 20](#_Toc455573395)

[10.3.2 Instruction cpu 20](#_Toc455573396)

[10.3.3 Stack 20](#_Toc455573397)

[10.4 Seven segment display 21](#_Toc455573398)

[10.4.1 Battery of 8 switches 21](#_Toc455573399)

[10.5 Toolbar 22](#_Toc455573400)

[1.1. Gui Menu 22](#_Toc455573401)

[11 Gui behaviour 23](#_Toc455573402)

[11.1 File types used in the simulator 23](#_Toc455573403)

[11.1.1 Files that could be used in the Simulator 23](#_Toc455573404)

[11.2 How to change memory value? 23](#_Toc455573405)

[12 Debugger 25](#_Toc455573406)

[12.1 Step Button 25](#_Toc455573407)

[12.2 Breakpoints 25](#_Toc455573408)

[12.3 – Run Button 25](#_Toc455573409)

[12.4 – Stop Button 25](#_Toc455573410)

[13 – Easy8 instructions list 25](#_Toc455573411)

[14 Appendix 27](#_Toc455573412)

[14.1 Save file flow 29](#_Toc455573413)

[15 CONCLUSIONS and future work 31](#_Toc455573414)

[16 Index 32](#_Toc455573415)

[List of pictures 33](#_Toc455573416)

# Introduction

The study of the Instruction Set Architecture is a very important subject in studies of computer design and programing

First year students cannot address on real processor because of its complexity and therefore more simple computers should be used. This is the case of the Easy8 computer. Although it is an educational and very simple computer, it includes the same components like real computers: CPU with registers, main memory, input/output system and a short but representative set of instructions.

# Objective

The goal of this project is to make a computer simulator of the Easy8 computer as defined in FCO subject Grade Engineering Technology and Telecommunication Services ETSIT.

It should be easy to use by the student, with low curve learning.

It should be possible to be used from many platforms.

It should include a graphical interface.

# Requirements

* Execution from windows/linux/unix.
* Execution of Join on basic assembler language with minimal set of instruction list.
* Work with ASM files, join them and reload them from the memory.
* Ability to stop/continue execution of the system.  
  Ability to add Breakpoints.
* Ability to have input/output to display/external system.  
  User interface to change memory.
* Load/save memory for working again on the same system.
* Show to the user the impact of the memory.
* Working with hexadecimal base

# Application design

The design of the application based on object oriented while using design patterns. Frameworks were used as much as possible. Java was the selected languages, as it gave the ability to be executed from many platforms.

AGILE was used as the methodology of the writing the code.

The TDD – Test driven development was in use , partially.

The application was done with java, as object oriented language. Some design patterns were in used, as described later in internal following list. The project was done in object oriented methodology. One exemplar to this could be the Seven Digits display – which wasn’t write from scratch, but used the Swing Panel and extends it.

Following framework was in used: Gui – Swing. JPanel, data model of JList were extended . XML - JAXB.

The implementation of the handling of the instructions in the logic model – was done with TDD – Test driven development.

Utils class was created as a Helper class which will include the methods that are not part of the Panel handling itself. It will shortly the code to be more viewable.

## Used design patterns

### Singleton pattern

The singleton pattern was used to create only one occurrence of every member of the CPU. LogicalCpu is the class of the Singleton. The singleton implementation was done with double checking to prevent entering double time on the same time.

### Factory Pattern

The factory pattern was used to create the required implementation of ActivityPiece in run time, for every step while execution the assembled code. Factory class name is ActivityPieceFactory.  
[[1]](#footnote-2)

## Pseudo codes

### Main - Run/Step execution

#nextAddress = getNextAddress()

#step()

#updatePc()

#Show impact memory fields

#Show next step on the Instruction CPU window

Explanation:

The execution method was built with the following steps:

1. Get the next instruction to be executed.
2. Execution of the step in the logic. For example: Pull data value by ref or immediately from the operand and put in the required place according to the Instruction.
3. Update the pc after the execution of the instruction.
4. Show the impact memory by the last command
5. Show the next step to be executed.

### Instruction implementation

The implementation of one instruction is built with the following pseudo code:

#updateModel()

#create new event for gui

#Create jump event

### Seven Digit display

# FOR INT numOfDigits <=2

# FOR int pieceNumber <=7

# Draw the piece ON/OFF [using the graphics.fillPolygon method]

### Pseudo code Explanations

1. The Gui would later go on list of received events and handling them to show impact memory, next command, new registers values.
2. Create Jump event – will update the CP to another value instead of using the address of the the next command.

## Customization of classes

1. JPanel – customized for display the Seven Digit
2. AbstractListModel – extends for adding some properties to the display of the List.

# Environment / Programming language/Implementation

This section contains the selected environment/languages and implementation of one object of the Simulator.

The development was done in Windows 7. NetBeans version 8.1 was the selected IDE for this Simulator. Maven was the build system.

The selected programing language was java as it’s give the ability to execute it on Windows/Linux.

The selected java version was 1.8.


## Implementations

### Seven digit

High level design:

The implementation of the seven digit display was done by extends the JPanel class of Swing. In the constructor of the panel we created list of polygons, every piece of the display is one polygon. Every number has list of On/OFF for the polygons. Select one value – get the required pieces that should be on and display them.

UML class diagram of class



Methods

getPreferredSize – used by the parent panel to create the customized panel with the required Size.

paintComponent - does the creation of the display.

Interface:

Creation – as in the following line, in the generated code:[[2]](#footnote-3)

sdPanel = new meirdev.simulator.gui.customized.panels.CPanelSevenDigit();

Update value – using the method setNumber to update the value.

### Battery of 8 switches

High level design:

Frame which contains 8 JCheckBox was created. One event handler was created for all of the array of the swing check box. The event handler was created for the stateHandler event. The Event handler use the method pullInValue for pulling the new value of the input and display it above the check boxes. When the value from the input is required – the methd pullInValue is used.

Methods

pullInValue – Walk on the list of check boxes and evaluate the integer value of the array.

extractValueFromInput – Builds a new string whoch contains ZERO for off and ONE for on.

paintComponent -No such method. Uses default implementation of the swing components.

Interface:

Creation – Uses the designer. Every check box was created as a regular check box.

Update value – No way to update the value of the checkboxes.

Pulling value of the switches = using the method pullInValue.

### Implementation of one instruction – we show here the instruction CALL

High level design:

The steps manager does the following activities:

* Fetches the command to be executed and set it as the current command.
* Execute the command. The execution uses the implementation of this command.
* The implementation of this command:
  + Handle the current command – insert the pc of the next command to the stack. [Logical section of the simulator]
  + Create a new event.

The gui does the following things:

* + - 1. Walk on list of events that are related to the Gui. No such event was created.
      2. Populate the event that was created and execute it. It will change the current pc to another one. It uses the jumpTo method of the StepManager.
    1. The gui will change the PC to the new PC.
    2. The gui will update the RA with the RA register.

# Configuration files

This section contains list of configuration issue.

Files

* Easy8Instructions.xml – internal in the jar. This file contains the list of the available instructions of the CPU.
  + File name: Easy8Instructions.xml.
  + File location: root of the jar.

Every command has the following details in his XML entity:

* + - 1. Attribute’s list of one entity:
         1. type – the type of the instruction. There are two types – one type has additional operand, second type do not have operand value.
         2. ov – NO for instruction with the type one\_word. Otherwise it should contains YES.
      2. List of OperationList.
         1. Instruction with some operation value would have the same name. Therefore, every operation value has one operationCode entity in the OperationList entity.
      3. operationCode
         1. Attributes:

ovValue1=type of operand.

* + - * 1. Value – the operation code of the instruction with the specific operand.
  + One change that could be done by overriding this file, without changing the code, is to replace the value of the operationCode, which contains the operation code of the assembler.

For example:

<operationCode>0x15</operationCode>

The value of 0x15 could be changed to another value,

# Joiner working

This section will describe the abilities of the joiner, process of the joiner, some of the errors..

The shell command receive input file according to the parameter of the java execution.

For example:

With the following command – it will join the file test.asm [the real command will be on the same line, so please do not care to the EOL which currently is inside the doc.]

java -cp SimEasy8-jar-with-dependencies.jar meirdev.simulator.simeasy8.AssemblerReader test.asm

In case that file wasn’t exists – it will display the error:

Parameter issue - file does not exist:[<full file name>]

So, the user should put the file according to the place which appeared in the error.

While the reading of the file:

No comment exists in the file.

Max size of the file is the memory available to this machine. Currently – the max memory which could be is 256. The reader will throw error when the number of lines will be more than 512.

In case of too many lines – the file contains more lines than 256 which is the size of instruction area – the following error will be shown:

Jun 20, 2016 6:25:55 PM meirdev.simulator.simeasy8.AssemblerReader verifyFileSizeSEVERE: The file contains too much lines. :[316]. The max number could be :256

In case that additional space was beteen the command and the operand, the following error will be viewed:

SEVERE: Assemble Error- Operand's command contains: :.[],MOVE RA,43, In line :2

Jun 20, 2016 7:00:11 PM meirdev.simulator.simeasy8.AssemblerReader assebleLines

The display of the error is only when the join was done in the shell.

In case of it will be done from the gui –



The error message will be disappeared only after the join will pass.

The join stops after the first error.

# Known Limitations-improvements

The following list contains the known limitation of the current version of the simulator.

The current system has limitations in the following items: Error handling of Assemble process, Seven digit update. [Verification of the limit of operand value]

* Error handling of asm file

The join process give good errors when the Join is done by the Shell/Cmd on Linux/Win systems. Please see in the manual the steps which should be done for compile asm file. When the join is done in the GUI – the errors will not be viewed.

* Seven digit update

The Seven-digit display regular definition exists only for regular decimal number. No display for the case that output value has one of the additional characters. Previous value will remain in case that RA contains value which has a characte which is part of hexdecimal base, instead of a number.

# Manual

This section describes the instruction how to execute system as gui/shell/cmd commands.

## Execution of Gui

|  |  |
| --- | --- |
| * + 1. Windows | 1. Extract the files to working directory. 2. Execute the Gui.bat |
| * + 1. Linux | 1. Extract the file to local folder. 2. Open the shell to this folder 3. Execute the following java command: 4. java -cp SimEasy8-jar-with-dependencies.jar meirdev.simulator.gui.frmae.GuiSimulator |

## Execution of joiner

|  |  |
| --- | --- |
| * + 1. Windows | 1. Extract the files to working directory. 2. Execute the Show.bat |
| * + 1. Linux | 1. Extract the file to local folder. 2. Open the shell to this folder 3. Execute the following java command: 4. java -cp SimEasy8-jar-with-dependencies.jar meirdev.simulator.simeasy8.AssemblerReader test.asm |

The last parameter for the java is the assembler file to be joined.

# Gui

In this section the GUI will be described. The gui has the following items:

Menu – Some activities that could be with the menu.

Commands bar – Main frequency activties

Editor – Editor for the joiner program

PC Memory – Display the memory values

Edit memory value – Frame for changing value of specific memory address

Instruction menu – This frame contains List of instructions after Assemble success. Also show the next instruction to be used

Output – Seven digit - display numbers in Seven digit type of display.

Processor registers – contains the registers of the CPU.

Processor flags

Stack – show the memory of the stack.

Message – on the top – show error of the join of the assembler.

Message []

## All parts view




Figure 1- Simulator parts

## Editing/saving assembler/memory files

- Edition frame to edit programs in assembly language.

### Open assembler file


The file will be opened as in the following image, using the File/Open menu item /Sub menu item. Only asm files will be viewed from this dialog window.



2Open file

### Save assembler file


Save file – Use the Save / Save as sub menu. Extention of the file name could be ignored in this activity.



3Save as - menu item q Sub menu item

Window (or frame) to display processor registers (PC, SP and RA) and outcome indicators (C, N, Z and V). These records will be updated either by the execution of the instructions or because the user modifies the content.

In the current version – the edit of the values is done currently in hexadecimal.




7Processor registers and outcome indicators.

## Memory view

### Memory

The memory is a frame which contains internally two lists, as in the following image:




We have here two sections:

* Left list – Contains counter from ZERO to 0XFF, display as hex decimal values[in the current image – from 15 to 22 where in decimal is from 21 to 34]
* Right list – contains the memory value. The format of the memory value is [11111111] (0xFF), while 11111111 are 8 bits of the value and 0xFF contains 2digits of HEX DECIMAL value.

The two list are joind so selection of one cell in one of the lists selects also the corresponding value in the second list.

### Instruction cpu

The instruction cpu is a frame which builts with two lists. The left one contains counter from ZERO to 0xFF. The right one contains the the address in two modes: when it’s with ‘\*’ – its not a starting place of an instruction.



### Stack

The same frame like for the memory, but will show the stack.

## Seven segment display

- A seven-segment display two digits to display the output of 0x01 OUT instruction (is as it is in the current simulator)

### Battery of 8 switches

- A battery of 8 switches, to generate the input to the instruction IN 0x00. The user must be able to change the position of each of the switches (on / off) with the mouse.


From the high bit at the top to the lower bit .

For example:

|  |  |
| --- | --- |
| Figure 8 battery of 8 switches - 4B value | Figure 9 0F value |

Figure 10 battery of 8 switches - 4B value

- A hexadecimal as having the current simulator keyboard, but instead of an OK button, you will have something like a push button (https://electrosome.com/wp-content/uploads/2012/12/Push-Button -Switch.jpg).



## Toolbar

- A panel with buttons (or bar, although I prefer panel with large buttons so you can read the function of each button) with the following buttons:

Assemble, Step (Step by Step Run) Run (Uninterruptible Execution), Reset PC (Set to 0 the PC), Reset RA (Reset the RA), Reset SP (Reset the SP), Reset memory ( Reset all memory) and RESET (Resets all of the above).

The RESET button in the tool bar will have confirmation, to prevent from reset by mistake.[[3]](#footnote-4)

STOP button

* 1. Gui Menu

Reset menu – all the reset options.

# Gui behaviour

Behavior of the different elements:

Used files in the Simulator

## File types used in the simulator

There are two file types which are used in the simulator:

### Files that could be used in the Simulator

The Simulator could work without any files. The files are only for storing/loading previous Assembler /memory files.

**ASM**

This type of file contains the assembler code.

Could be loaded from param when execution is from console or by Menu item when execution is done by the Gui.

The format of the file is ascii, separated by colon

**MEM**

This type of file contains the memory code.

The format of the file is ascii, separated by colon

-buttons Reset PC, RA, SP and memory.

These buttons reset the corresponding record (or all memory). The outcome indicators are reset in conjunction with RA or when reset everything.

Assembler –button

Once introduced into an assembly program editor, the simulator must analyze it to translate into machine code. If an error is detected, for example, the instruction does not exist or is missing an operand, display an error message and indicate where the error occurred. It takes no great sophistication, as the language is simple and regular.

If no errors are loaded into memory the result of code the program into machine code.

## How to change memory value?

Use one of the following ways to change the value of the memory:

* 1. Click on the selected memory value
     1. One click – change the selected memory value, and change also the selected address in the Yellow qube
     2. Double click – Move the focus of the frame to the input holding the new value of the memory, after the selected address already changed to the correct address.
  2. Change the slider “val” of the memory value.

The value which appears on the input is the decimal value, on the memory itself – it’s appeared in hex decimal value.

# Debugger

This section describes the options of the exection/debugger of the Simulator.

## Step Button

Execute the instruction pointed to by the PC and stop updating all the graphics and state of the computer elements.

## Breakpoints

The user could add break point in the required address.

Note:Breakpoint could be added only after finished of assemble activity.



## Run Button

Execute the instruction pointed to by the PC, update the machine status and graphic elements, and continue with the next instruction. The execution will stop when it reaches the Stop instruction or press the STOP button.

## Stop Button

Stops program execution.

# 

# Easy8 instructions list

**This section show the list of instructions exist in the Easy8.**

* When command ends with the char: ‘I’it means that it will populate the value in the second operator and use it to the specific instruction.
* MOVEI RA, VALUE
* MOVR RA,25
* MOVE 34,RA
* ADDI RA,34
* ADD RA, 45
* SUBI RA,V 56
* SUB RA,46
* INC RA
* DEC RA
* COMPAREI RA, VALUE
* COMPARE RA, VALUE
* JUMP ADDRESS
* JLESS ADDRESS
* JGREATER ADDRESS
* JEQUAL ADDRESS
* PUSH RA
* POP RA
* CALL ADDRES
* RET

# Appendix

* This section will give two assembler files: One with IO Out and one with IO IN. The flow of save will be displayed here also.

Assembler program with IO

**Basic flow – output to the Seven digit**

This flow will display Hex 77 in the Seven Digit output.

The following steps should be done to work with ASM file.

The display of the seven digit for the default value will be as in the following image:




Figure 11Seven digit contain default value

1. Load ASM file with Open file menu/Sub menu
2. Edit the file in the Editor section
3. Clear the contents of the editor
4. Add the following lines:
   1. OUT 77
   2. STOP




Figure 12Editie -ASM lines to display 77 in the seven digit

1. Assemble the file.
2. Run the assembled code.





Figure 13Seven digit in the ending of the execution - hex 77

**Basic flow – Input from the seven switches battery**

The following steps should be done to work with ASM file.


The Battery switch list should be as in the following image:

(Only value that has only regular digits will be displayed in the Seven Digit display)




1. Clear the contents of the editor
2. Add the following lines:
   1. IN 5
   2. OUT 77
   3. STOP
3. Assemble the file.
4. Run the assembled code.

The following image, contains the registers as they are appeared in the end of the program:


 

The instruction list will be as in the folowing image




## Save file flow


Saving the file name with no extension, will save the file with the correct extension, as in the following pictures. The result is – that open file will view the file and file will be opened with no issues:



4save asm file - test5 - with no extension



5The file was saved corectly - as test5.asm[Viewdlated by the open file ]



6Editor window

The editor window – contains window with editor for the ASM code.

# CONCLUSIONS and future work

This work is basic simulator with very simple input/output.

Additional improvements - already exist in another section.

New features could be storing the asm file in the internet, grouped by classes.

Programing improvements – could be do the next step and split the code of the logical model and the GUI itself, so another model could be used.

Comment

For adding a new command – one existing command should be removed.

# Index

Execution: Asseble of asm file, 15

Seven Digit: comment, 27

List of pictures

[Figure 1Seven digit contain default value - 00](#Toc453325212) 30

[Figure 2Editie -ASM lines to display 77 in the seven digit](#Toc453325213) 30

[Figure 3Seven digit in the ending of the execution - hex 77](#Toc453325214) 30

[Figure 4Seven digit contain default value - 00](#Toc453325215) 31

[Figure 5Seven digit in the ending of the execution - hex 77](#Toc453325216) 31

[Figure 6- Simulator parts](#Toc453325217) 18

[7Open file](#Toc453325218) 19

[8Save as - menu item q Sub menu item](#Toc453325219) 19

[9save asm file - test5 - with no extension](#Toc453325220) 20

[10The file was saved corectly - as test5.asm[Viewdlated by the open file ]](#Toc453325221) 20

[11Editor window](#Toc453325222) 21

[12Processor registers and outcome indicators.](#Toc453325223) 21

[Figure 13 battery of 8 switches - 4B value](#Toc453325224) 24

[Figure 14 0F value](#Toc453325225) 24

[Figure 15 battery of 8 switches - 4B value](#Toc453325226) 2

1. The decision which implementation to create is done according to the input which contains the command, In the run time assumption is taken that current instruction is exist [after assemble has been pass already before] [↑](#footnote-ref-2)
2. NetBeans add the customized creation code. The component has ***Custom creation code*** in the Code properties tab. [↑](#footnote-ref-3)
3. The reset menu – do not have this option. It’ [↑](#footnote-ref-4)